


## Case Study 02: Usage of meta-arg

**VPC**





**Subnets**






**Route table**







**Internet Gateway**



**Elastic IP**



**Public Subnet NAT**



**Security Group**

